{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["１","２ "],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"１","index":0,"n_rows":46,"n_cols":7,"rows_kept":46,"cut":false,"hidden":false,"merged":[[42,1,42,2],[42,3,42,4],[42,5,42,8],[43,1,43,2],[43,3,43,8],[45,6,45,8],[40,1,40,2],[40,3,40,4],[40,5,40,8],[41,1,41,2],[41,3,41,4],[41,5,41,8],[37,1,37,2],[37,3,37,8],[38,1,38,2],[38,3,38,8],[39,1,39,2],[39,3,39,4],[39,5,39,8],[32,1,32,8],[33,1,36,2],[33,3,33,8],[34,3,34,8],[35,3,35,8],[36,3,36,8],[28,2,28,4],[28,6,28,8],[29,2,29,4],[29,6,29,8],[30,1,30,8],[31,1,31,8],[25,2,25,4],[25,6,25,8],[26,2,26,4],[26,6,26,8],[27,2,27,4],[27,6,27,8],[20,6,20,8],[21,2,21,8],[22,1,26,1],[22,2,22,4],[22,5,26,5],[22,6,22,8],[23,2,23,4],[23,6,23,8],[24,2,24,4],[24,6,24,8],[16,1,20,1],[16,2,16,5],[16,6,16,8],[17,2,17,5],[17,6,17,8],[18,2,18,5],[18,6,18,8],[19,2,19,5],[19,6,19,8],[20,2,20,5],[10,1,10,8],[11,1,11,8],[12,1,12,8],[13,1,13,8],[14,1,14,8],[15,1,15,5],[15,6,15,8],[6,1,6,8],[7,1,7,8],[8,1,8,8],[9,1,9,8],[0,1,0,9],[1,1,1,9]],"flags":["formulas_cached_only"]}
[null,"＊＊＊　模拟计算委托书　＊＊＊"]
[null,"（间歇蒸馏用/已建改造）"]
[]
[{"$nulls":5},"Date    :"]
[{"$nulls":5},"Item No :"]
[{"$nulls":5},"機器名称 : "]
[null,"目的"]
[]
[]
[]
[null,"工程的概要（用骨架图图示说明等）"]
[]
[]
[]
[null,"设计规格"]
[null,"塔顶压力 (mmHga　、kg/cm2G　、kpaG　、kpaA)　 ※请划○"]
[null,"处理液　　　　　　　　　　　　　　　　　　　　　　","组成：",null,null,null,"处理液量(kg)："]
[null,null,"组成：",null,null,null,"处理液量(kg)："]
[null,null,"组成：",null,null,null,"处理液量(kg)："]
[null,null,"组成：",null,null,null,"处理液量(kg)："]
[null,null,"组成：",null,null,null,"处理液量(kg)："]
[null,"总处理液量(kg)"]
[null,"留出组成",null,null,null,"处理液残量组成"]
[]
[]
[]
[]
[null,"留出（环流）量(kg/hr)",null,null,null,"处理液残量(kg/hr)"]
[null,"留出（环流）温度（℃）"]
[null,"１个间歇时间(hr)"]
[null,"　　※１个间歇时间：请从初留、留出开始时计时"]
[null,"　　　　不包括放进蒸留原料所需要时间、升温时间、全环流时间、及留出停止后的Hold up液＋放出处理液的时间"]
[null,"分离条件（具体的）"]
[null,"要求SPEC　　　　　　　　　　　　　　　　　　　　　　　　"]
{"$rows_empty":11}
[null,"Ver2 29.JAN.13'",{"$nulls":4},"Matsui Machine Ltd."]

{"sheet":"２ ","index":1,"n_rows":46,"n_cols":10,"rows_kept":46,"cut":false,"hidden":false,"merged":[[43,1,43,9],[44,1,44,9],[45,7,45,9],[37,1,37,9],[38,1,39,2],[38,3,38,9],[40,1,40,2],[41,1,41,2],[42,1,42,9],[32,1,35,2],[32,3,32,9],[33,3,33,9],[34,3,34,9],[35,3,35,9],[36,1,36,2],[36,3,36,6],[36,7,36,9],[28,7,28,9],[29,4,29,6],[29,7,29,9],[30,4,30,6],[30,7,30,9],[31,1,31,9],[24,4,24,6],[24,7,24,9],[25,1,30,1],[25,4,25,6],[25,7,25,9],[26,4,26,6],[26,7,26,9],[27,4,27,6],[27,7,27,9],[28,4,28,6],[21,4,21,6],[21,7,21,9],[22,4,22,6],[22,7,22,9],[23,4,23,6],[23,7,23,9],[16,1,16,2],[16,3,16,9],[17,1,17,9],[18,4,18,6],[18,7,18,9],[19,1,24,1],[19,4,19,6],[19,7,19,9],[20,4,20,6],[20,7,20,9],[14,1,14,2],[14,3,14,5],[14,6,14,9],[15,1,15,2],[15,3,15,5],[15,6,15,9],[12,1,12,2],[12,3,12,5],[12,6,12,9],[13,1,13,2],[13,3,13,5],[13,6,13,9],[9,1,9,2],[9,3,9,9],[10,1,10,2],[10,3,10,9],[11,1,11,2],[11,3,11,9],[6,1,6,2],[6,3,6,9],[7,1,7,2],[7,3,7,5],[7,6,7,9],[8,1,8,2],[8,3,8,5],[8,6,8,9],[0,1,0,9],[1,1,1,9],[3,1,3,9],[4,1,4,2],[4,3,4,9],[5,1,5,2],[5,3,5,5],[5,6,5,9]],"flags":["formulas_cached_only"]}
[null,"＊＊＊　模拟计算委托书　＊＊＊"]
[null,"（间歇蒸馏用/已建改造）"]
[]
[null,"其他"]
[null,"运转操作范围 （Min ～ Max）",null,"％　　　　　　　　　　　　～　　　　　　　　　　％"]
[null,"冷凝器的有无",null,"有　　　　　　无",null,null,"　出口温度　：　"]
[null,"重沸器的有无",null,"有　　　　　　　　　　　　　　　　　　　　　　　无"]
[null,"塔底吹气口的有无",null,"有　　　　　　无",null,null,"　出口温度、压力　：　"]
[null,"塔内容许压降",{"$nulls":4},"　单位　： (mmHg、mmH2O、kpaA) 　※请划○"]
[null,"２液层的可能性的有无",null,"有　　　　　　　　　　　　　　　　　　　　　　　　无"]
[null,"填料的材质"]
[null,"塔内件材质"]
[null,"塔体材质",{"$nulls":4},"　设计温度＆设计压力　：　"]
[null,"塔体适用法规",{"$nulls":4},"　支持方法　：　"]
[null,"起泡的有无",null,"有　　　　　　无",null,null,"　起泡因子　：　"]
[null,"污垢的有无",null,"有　　　　　　无",null,null,"　具体的　：　"]
[null,"其他、现运转中的问题点等"]
[null,"既设塔规格"]
[null,null,"部位","填充高度","填料种类・尺寸",null,null,"材质"]
[null,"浓缩部","1st BED"]
[null,null,"2nd BED"]
[null,null,"3rd BED"]
[null,null,"4th BED"]
[null,null,"5th BED"]
[null,null,"塔内件"]
[null,"回收部","1st BED"]
[null,null,"2nd BED"]
[null,null,"3rd BED"]
[null,null,"4th BED"]
[null,null,"5th BED"]
[null,null,"塔内件"]
[null,"分离条件（具体的）"]
[null,"要求SPEC　　　　　　　　　　　　　　　　　　　　　　　　"]
[]
[]
[]
[null,"理论板",{"$nulls":5},"环流比："]
[null,"其他"]
[null,"贵司实绩值　　　　　　　　　　　　　　　　　　　　　　　　　　　　　（作为参考请告知）",null,"间歇时间"]
[null,null,null,"１小时后","2小时后","３小时后","４小时后","５小时后","６小时后","７小时后"]
[null,"环流量(m3/hr)"]
[null,"环流比"]
[]
[null,"※请提出既设塔体图纸、及塔内件详细图纸"]
[]
[null,"Ver2 29.JAN.13'",{"$nulls":5},"Matsui Machine Ltd."]