{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["１","２ "],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"１","index":0,"n_rows":46,"n_cols":7,"rows_kept":46,"cut":false,"hidden":false,"merged":[[42,1,42,2],[42,3,42,4],[42,5,42,8],[43,1,43,2],[43,3,43,8],[45,6,45,8],[40,1,40,2],[40,3,40,4],[40,5,40,8],[41,1,41,2],[41,3,41,4],[41,5,41,8],[37,1,37,2],[37,3,37,8],[38,1,38,2],[38,3,38,8],[39,1,39,2],[39,3,39,4],[39,5,39,8],[32,1,32,8],[33,1,36,2],[33,3,33,8],[34,3,34,8],[35,3,35,8],[36,3,36,8],[28,6,28,8],[29,2,29,4],[29,6,29,8],[30,2,30,4],[30,6,30,8],[31,2,31,4],[31,6,31,8],[24,2,24,4],[24,5,24,7],[25,1,25,8],[26,1,30,1],[26,2,26,4],[26,5,30,5],[26,6,26,8],[27,2,27,4],[27,6,27,8],[28,2,28,4],[20,6,20,8],[21,2,21,4],[21,6,21,8],[22,2,22,4],[22,6,22,8],[23,2,23,8],[16,1,16,8],[17,1,21,1],[17,2,17,4],[17,5,21,5],[17,6,17,8],[18,2,18,4],[18,6,18,8],[19,2,19,4],[19,6,19,8],[20,2,20,4],[10,1,10,8],[11,1,11,8],[12,1,12,8],[13,1,13,8],[14,1,14,8],[15,1,15,5],[15,6,15,8],[0,1,0,8],[1,1,1,8],[6,1,6,8],[7,1,7,8],[8,1,8,8],[9,1,9,8]],"flags":["formulas_cached_only"]}
[null,"＊＊＊  模拟计算委托书　＊＊＊"]
[null,"（吸收用/已建改造）"]
[]
[{"$nulls":5},"Date     :"]
[{"$nulls":5},"Item No  :"]
[{"$nulls":5},"機器名称  : "]
[null,"目的"]
[]
[]
[]
[null,"工程的概要（用骨架图图示说明等）"]
[]
[]
[]
[null,"设计规格"]
[null,"塔顶压力 (mmHga　、kg/cm2G　、kpaG　、kpaA)　 ※请划○"]
[null,"液体侧条件 (ppm的时候、请记载wt或vol）"]
[null,"入口",null,null,null,"出口                             （放散SPEC）　　　　　　　　　　　　　　　　　"]
[]
[]
[]
[]
[null,"液体流量(kg/hr)",null,null,null,"温度(℃)"]
[null,"吸收液名称"]
[null,"液流量的上限值的有无","有　　　　　　　无",null,null,"　上限值 (kg/hr、m3/hr)　※请划○　： "]
[null,"气体侧条件 (ppm的时候、请记载wt或vol）"]
[null,"入口",null,null,null,"出口                             （吸収SPEC）　　　　　　　　　　　　　　　　　"]
[]
[]
[]
[]
[null,"气体(kg/hr)",null,null,null,"温度(℃)"]
[null,"吸收（放散）条件（具体的）"]
[null,"要求SPEC　　　　　　　　　　　　　　　　　　　　　　　　"]
{"$rows_empty":11}
[null,"Ver2 29.JAN.13'",{"$nulls":4},"Matsui Machine Ltd."]

{"sheet":"２ ","index":1,"n_rows":46,"n_cols":7,"rows_kept":46,"cut":false,"hidden":false,"merged":[[43,1,43,9],[44,1,44,8],[45,6,45,8],[38,1,38,2],[38,4,38,5],[38,7,38,8],[39,1,42,2],[39,3,39,8],[40,3,40,8],[41,3,41,8],[42,3,42,8],[33,1,36,2],[33,3,33,8],[34,3,34,8],[35,3,35,8],[36,3,36,8],[37,1,37,2],[37,3,37,8],[29,6,29,8],[30,4,30,5],[30,6,30,8],[31,4,31,5],[31,6,31,8],[32,1,32,8],[25,4,25,5],[25,6,25,8],[26,1,31,1],[26,4,26,5],[26,6,26,8],[27,4,27,5],[27,6,27,8],[28,4,28,5],[28,6,28,8],[29,4,29,5],[22,4,22,5],[22,6,22,8],[23,4,23,5],[23,6,23,8],[24,4,24,5],[24,6,24,8],[17,1,17,2],[17,3,17,8],[18,1,18,8],[19,4,19,5],[19,6,19,8],[20,1,25,1],[20,4,20,5],[20,6,20,8],[21,4,21,5],[21,6,21,8],[15,1,15,2],[15,3,15,4],[15,5,15,8],[16,1,16,2],[16,3,16,4],[16,5,16,8],[12,1,12,2],[12,3,12,8],[13,1,13,2],[13,3,13,4],[13,5,13,8],[14,1,14,2],[14,3,14,4],[14,5,14,8],[9,1,9,2],[9,3,9,4],[9,5,9,8],[10,1,10,2],[10,3,10,8],[11,1,11,2],[11,3,11,8],[6,1,6,2],[6,3,6,4],[6,5,6,8],[7,1,7,2],[7,3,7,8],[8,1,8,2],[8,3,8,4],[8,5,8,8],[0,1,0,8],[1,1,1,8],[3,1,3,8],[4,1,4,2],[4,3,4,8],[5,1,5,2],[5,3,5,8]],"flags":["formulas_cached_only"]}
[null,"＊＊＊  模拟计算委托书　＊＊＊"]
[null,"（吸收用/已建改造）"]
[]
[null,"其他"]
[null,"液体测运转操作范围（Min ～ Max）",null,"％　　　　　　　　　　　　～　　　　　　　　　　％"]
[null,"气体侧运转操作范围 （Min ～ Max）",null,"％　　　　　　　　　　　　～　　　　　　　　　　％"]
[null,"冷凝器的有无",null,"有　　　　　　无",null,"　出口温度　：　"]
[null,"リボイラ－の有无",null,"有　　　　　　　　　　　　　　　　　　　　　　　　无"]
[null,"塔底吹气口的有无",null,"有　　　　　　无",null,"　出口温度、圧力　：　"]
[null,"塔内容许压降",null,null,null,"　单位　： (mmHg、mmH2O、kpaA) 　※请划○"]
[null,"２液层的可能性的有无",null,"有　　　　　　　　　　　　　　　　　　　　　　　　无"]
[null,"填料的材质"]
[null,"塔内件材质"]
[null,"塔体材质",null,null,null,"　设计温度＆设计压力　：　"]
[null,"塔体适用法规",null,null,null,"　支持方法　：　"]
[null,"起泡的有无",null,"有　　　　　　无",null,"　起泡因子　：　"]
[null,"污垢的有无",null,"有　　　　　　无",null,"　具体的　：　"]
[null,"其他、现运转中的问题点等"]
[null,"既设塔规格"]
[null,null,"部位","填充高度","填料种类・尺寸",null,"材质"]
[null,"浓缩部","1st BED"]
[null,null,"2nd BED"]
[null,null,"3rd BED"]
[null,null,"4th BED"]
[null,null,"5th BED"]
[null,null,"塔内件"]
[null,"回收部","1st BED"]
[null,null,"2nd BED"]
[null,null,"3rd BED"]
[null,null,"4th BED"]
[null,null,"5th BED"]
[null,null,"塔内件"]
[null,"现状吸收（放散）条件（具体的）"]
[null,"要求SPEC　　　　　　　　　　　　　　　　　　　　　　　　"]
[]
[]
[]
[null,"理论板"]
[null,"移动单位高度　及　移动单位数",null,"Hog",null,null,"Nog"]
[null,"其他"]
[]
[]
[]
[null,"※请提出既设塔体图纸、及塔内件详细图纸"]
[]
[null,"Ver2 29.JAN.13'",{"$nulls":4},"Matsui Machine Ltd."]